{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["KALKULATOR"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"KALKULATOR","index":0,"n_rows":32,"n_cols":19,"rows_kept":32,"cut":false,"hidden":false,"merged":[[26,1,31,1],[15,9,15,10],[11,1,13,1],[11,2,13,2],[11,3,11,6],[13,3,13,6],[14,1,19,1],[20,1,25,1]]}
["Dobór podnośników gazowych",null,null,null,null,null,null,null,"Dobór podnośników TOP STAYS"]
[null,null,null,null,null,null,null,null,null,null,null,"F = "]
[]
[]
[null,"Kąt otwarcia: ",null,"Kąt otwarcia: ",null,null,null,null,null,"Wysokość frontu: ",null,"Wysokość frontu: ",null,null,null,null,null,null,"75°"]
[null,"Wysokość drzwi: ",null,"Wysokość drzwi: ",null,null,null,null,null,"Waga frontu: ",null,"Szerokość frontu: ",null,null,null,null,null,null,"90°"]
[null,"Waga drzwi: ",null,"Szerokość drzwi: ",null,null,null,null,null,"Waga uchwytu: ",null,"Grubość frontu: ",null,null,null,null,null,null,"105°"]
[null,null,null,"Grubość drzwi: ",null,null,null,null,null,null,null,"Materiał: "]
[null,null,null,"Materiał: ",null,null,null,null,null,null,null,"Waga uchwytu: ",null,null,null,null,null,null,"płyta wiórowa"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"płyta MDF"]
[]
[null,"Kąt otwarcia drzwi","Siła podnośika","Wysokość drzwi (mm)",null,null,null,null,null,"Wysokość frontu: ",null,"Współczynnik F",null,"Sprężyna","Biały","Szary"]
[null,null,null,300,400,500,600,null,null,"od","do","od","do"]
[null,null,null,"Waga drzwi (kg)",null,null,null,null,null,250,400,580,1250,"słaba","PD-LIFT-LIGHT-10","PD-LIFT-LIGHT-80"]
[null,"75°",50,1.6,1.2,1,0.8,null,null,400,500,960,2040,"średnia","PD-LIFT-MEDIUM-10","PD-LIFT-MEDIUM-80"]
[null,null,60,2,1.5,1.2,1,null,null,"500 mm",null,1080,3500,"mocna","PD-LIFT-STRONG-10","PD-LIFT-STRONG-80"]
[null,null,80,2.7,2,1.6,1.4]
[null,null,100,3.3,2.5,1.9,1.6]
[null,null,120,4,3,2.4,2]
[null,null,150,4.7,3.5,2.9,2.4]
[null,"90°",50,1.5,1.1000000000000001,0.9,0.7]
[null,null,60,1.8,1.3,1.1000000000000001,0.9]
[null,null,80,2.4,1.8,1.4,1.2]
[null,null,100,3,2.2000000000000002,1.8,1.5]
[null,null,120,3.6,2.7,2.1,1.8]
[null,null,150,4.3,3.2,2.6,2.1]
[null,"105°",50,1.3,0.9,0.8,0.6]
[null,null,60,1.6,1.2,0.9,0.8]
[null,null,80,2.1,1.6,1.2,1]
[null,null,100,2.6,1.9,1.6,1.3]
[null,null,120,3.1,2.2999999999999998,1.9,1.6]
[null,null,150,3.5,2.6,2.2000000000000002,1.9]